CAREL – Confidential



**REQUIREMENTS SPECIFICATION**

CloudGateMini

PLCM 9718

rev. See history

Index

[Index 2](#_Toc62111250)

[1 Revision 3](#_Toc62111251)

[2 Introduction 4](#_Toc62111252)

[2.1 Scope of the document 4](#_Toc62111253)

[2.2 Definitions, acronyms and abbreviations 4](#_Toc62111254)

[3 Improvement of the web server graphic interface 5](#_Toc62111255)

[3.1 Preface 5](#_Toc62111256)

[3.2 File contents 5](#_Toc62111257)

[3.3 Flow of a full file transfer 7](#_Toc62111258)

1. Revision

|  |  |  |  |
| --- | --- | --- | --- |
| Rev. | Rev. date | Author | Note |
| *0.1* | 17/09/2021 | A.Chiebao | 1st draft |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

1. Introduction
   1. Scope of the document

This document refers to the realization of some enhancement to the current FW of the CloudGateMini (this improvement will only affect the GTW000MWT0).

* 1. Definitions, acronyms and abbreviations

AP = WiFi access point to connect to

CGM\_AP = gateway that act as an access point  
CGM\_WIFI = CloudGateMini WiFi

CGM = CloudGateMini  
GSM = refer to 2G/4G/NB IoT connection  
FW = firmware

IoT = Internet of Things

MonDev = the device connected to the GME through the RS485 interface

OTA = Over The Air

SW = software  
MFT = Modbus File Transfer

GTW000MWT0 = the GME-WiFi model

GTW000MGP0 = the GME-2G model with CAREL SIM installed

GTW000MGT0 = the GME-2G model without SIM

GTW000M2W0 = the GME-2G+WiFi model without SIM

1. Improvement of the web server graphic interface
   1. Preface

The request is to make the configuration web pages exposed by the gateway more "friendly" to the customer. To do this it is necessary modify some files (.c/.h) on the firmware side, and also the .html files that generate the web pages.

It was also asked to make the debug page accessible (previously hidden and not directly available by the customer).

The following points detail the various changes required.

* 1. File contents